$#+Digital Semiconductor's 21X4 PCI Ethernet Controller Family

21040
21041
21140
21142
21143
EB40
EB41
EB140
EB142
EB143
MULTIA

$#+Digital Semiconductor's 21040 PCI Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation's Digital Semiconductor's 21040 based Adapter.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+Digital Semiconductor's 21041 PCI Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation's Digital Semiconductor's 21041 based Adapter.

AutoSense
AutoSense No_Nway
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+Digital Semiconductor's 21140 PCI Fast Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation's Digital Semiconductor's 21140 based Adapter.

AutoSense
AutoSense No_Nway
100BaseTx
100BaseTx Full_Duplex
100BaseT4
100BaseFx
10BaseT
10BaseT Full_Duplex

$#+Digital Semiconductor's 21142 PCI Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation's Digital Semiconductor's 21142 based Adapter.

AutoSense
100BaseTx
100BaseTx Full_Duplex
100BaseT4
100BaseFx
10BaseT
10BaseT Full_Duplex
10BaseT No_Link_Test
10Base2 (BNC)
10Base5 (AUI)

$#+Digital Semiconductor's 21143 PCI Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation's Digital Semiconductor's 21143 based Adapter.

AutoSense
100BaseTx
100BaseTx Full_Duplex
100BaseT4
100BaseFx
10BaseT
10BaseT Full_Duplex
10BaseT No_Link_Test
10Base2 (BNC)
10Base5 (AUI)

$#+EB40 - Digital Semiconductor's 21040's Evaluation Board
Use this dialog box to setup the medium connection for Digital Equipment Corporation's EB40 Evaluation Board.

Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test

$#+EB41 - Digital Semiconductor's 21041's Evaluation Board
Use this dialog box to setup the medium connection for Digital Equipment Corporation's EB41 Evaluation Board.

AutoSense
AutoSense No_Nway 
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+EB140 - Digital Semiconductor's 21140's Evaluation Board
Use this dialog box to setup the medium connection for Digital Equipment Corporation's EB140 Evaluation Board.

AutoSense
100BaseTx
100BaseTx Full_Duplex
10BaseT
10BaseT Full_Duplex

#+EB142 - Digital Semiconductor's 21142's Evaluation Board
Use this dialog box to setup the medium connection for Digital Equipment Corporation's EB142 Evaluation Board.

AutoSense
100BaseTx
100BaseTx Full_Duplex
100BaseT4
100BaseFx
10BaseT
10BaseT Full_Duplex
10BaseT No_Link_Test
10Base2 (BNC)

#+EB143 - Digital Semiconductor's 21143's Evaluation Board
Use this dialog box to setup the medium connection for Digital Equipment Corporation's EB143 Evaluation Board.

AutoSense
100BaseTx
100BaseTx Full_Duplex
100BaseT4
100BaseFx
10BaseT
10BaseT Full_Duplex
10BaseT No_Link_Test
10Base2 (BNC)

$#+DEC multia's Ethernet Controller 
Use this dialog box to setup the medium connection for Digital Equipment Corporation multia's Ethernet Controller.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+ DEC DE434 EtherWORKS Turbo PCI TP Adapter
Use this dialog box to setup the medium connection for Digital Equipment Corporation's DE434 EtherWORKS Turbo PCI TP Adapter.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test

$#+ DEC DE435 EtherWORKS Turbo PCI Adapter
Use this dialog box to setup the medium connection for Digital Equipment Corporation's DE435 EtherWORKS Turbo PCI Adapter.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+ DEC DE436 EtherWORKS Turbo PCI Quad Adapter
Use this dialog box to setup the medium connection for Digital Equipment Corporation's DE436 EtherWORKS Turbo PCI Quad Adapter.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test

$#+ DEC DE450 EtherWORKS Turbo PCI Adapter
Use this dialog box to setup the medium connection for Digital Equipment Corporation's DE450 EtherWORKS Turbo PCI Adapter.

AutoDetect
Twisted_Pair (10BaseT)
Twisted_Pair Full_Duplex
Twisted_Pair No_Link_Test
BNC (10Base2)
AUI (10Base5)

$#+ DEC DE500 FastEtherWORKS Turbo PCI Adapter
Use this dialog box to setup the medium connection for Digital Equipment Corporation's DE500 FastEtherWORKS Turbo PCI Adapter.

AutoSense
100BaseTx
100BaseTx Full_Duplex
10BaseT
10BaseT Full_Duplex

$#+Check once the 10BaseT (TP), 10Base2 (BNC) and 10Base5 (AUI) media ports and select the first live media. 
This detection takes place during driver initialization: the wire should be connected before the system boots and media  cannot be switched during run time.
AutoDectect does not check 10BaseT's Full_Duplex and No_Link_Test modes.

$#+Autosense the media ports supported by the Adapter and dynamically switch to the live media.
(AutoSense does not sense 10BaseT's No_Link_Test mode.)

$#+Autosense the media ports supported by the Adapter and dynamically switch to the live media.
Nway's negociation is disabled.
(AutoSense no_Nway does not sense 10BaseT's No_Link_Test mode.)

$#+Select the 10BaseT medium connection (RJ connector).

$#+Select the 10BaseT Full_Duplex medium connection (RJ connector).

$#+Select the 10BaseT medium connection (RJ connector) with no Link Integrity Test.
Choose this option if the Adapter is connected to a hub which does not generate link pulses to check the link integrity.

$#+Select the 10Base2 medium connection (BNC connector).

$#+Select the 10Base5 medium connection (AUI 15_pin connector).

$#+Select the Fast Ethernet 100BaseTx medium connection (RJ connector).

$#+Select the Fast Ethernet 100BaseTx Full_Duplex medium connection (RJ connector).

$#+Select the Fast Ethernet 100BaseT4 medium connection (RJ connector).

$#+Select the Fast Ethernet 100BaseFx medium connection.