# $ K + HP JetAdmin Utility

The HP JetAdmin utility is an administrative tool used to install and configure Hewlett-Packard printers connected to a network using an HP JetDirect print server (network interface). The HP JetAdmin utility operates as a Microsoft Windows utility and can be used for networking when a Novell NetWare server is available or with Peer-to-Peer networking in Microsoft Windows 95. It also allows users to monitor the current status of the printer.

{bmc LINE.BMP}

# $ K + To View the Graphical Printer Status
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the Printer tab.
A graphical representation of the printer status is shown in the upper-left corner of the page. 
3	Click OK when you are finished.

{bmc LINE.BMP}

# $ K Graphical Printer Status
Displays a graphical representation of the current printer status. The following list of conditions are described by the graphics:

{bmc BLTBLK.BMP}	Cover Open 
{bmc BLTBLK.BMP}	Output Bin Full 
{bmc BLTBLK.BMP}	Paper Jam 
{bmc BLTBLK.BMP}	Paper Out 
{bmc BLTBLK.BMP}	Toner Low 
{bmc BLTBLK.BMP}	JetDirect/EX Disconnected 
{bmc BLTBLK.BMP}	Printer Error 

{bmc LINE.BMP}

# $ K Cover Open
The printer's top cover is open, the toner cartridge is missing, or the cooling fan is not working.
Make sure the top cover of the printer is securely closed, the toner cartridge is installed, and the fan is operating.

{bmc LINE.BMP}

# $ K Output Bin Full
The output bin is full.
Remove paper from the output bin to resume printing.

{bmc LINE.BMP}

# $ K Paper Jam
A paper jam occurred.
Clear the paper jam. See the printer documentation for more information on clearing paper jams.

{bmc LINE.BMP}

# $ K Paper Out
The printer is currently out of paper, or the paper tray is not installed correctly.
Fill and reinstall the paper tray.

{bmc LINE.BMP}

# $ K Toner Low
The toner cartridge is low.
Try shaking the toner cartridge. Replace the toner cartridge in the near future.

{bmc LINE.BMP}

# $ K JetDirect/EX Disconnected
The parallel cable is not connected or not correctly connected.
Verify the cable is connected correctly. If the problem persists, contact your network administrator.

{bmc LINE.BMP}

# $ K Printer Error
An printer error occurred. This may be due to a page protection condition within the printer, an out of memory condition, or out of paper.
See the status section of this window for the current printer status and the printer message currently displayed on the printer. See the printer documentation for more information on the error.

{bmc LINE.BMP}

# $ K Busy
The internal communication channel of the printer subsystem is busy. If this continues, turn the printer OFF, then back ON.

{bmc LINE.BMP}

# $ K Online
The printer is online and ready to print.

{bmc LINE.BMP}

# $ K Printing
The printer is printing. 

{bmc LINE.BMP}

# $ K Printing Test Page
The printer is in the process of generating and printing a self-test page or configuration plot.

{bmc LINE.BMP}

# $ K Initializing
The HP JetDirect print server is initializing itself on the network.
When the printer is first turned on, the HP JetDirect print server must determine the protocol used on the network. Wait a few moments, then try sending the print job again.

{bmc LINE.BMP}

# $ K Offline
The printer is offline. Press the On Line key on the printer control panel to return the printer online and allow the printer to process print jobs.

{bmc LINE.BMP}

# $ K Out of Memory
Insufficient memory was available to process the print job. 
To prevent this error condition, reduce the complexity of graphics, remove soft fonts, simplify the print job, or add additional memory to the printer.

{bmc LINE.BMP}

# $ K Page Protection Needed
Insufficient memory was available to process the print job.
Set the printer or driver to the suggested page protection setting. 
See the printer documentation for more information on page protection.

{bmc LINE.BMP}

# $ K No Toner Cartridge
The toner cartridge is not installed in the printer. 
Complete the installation process for the selected printer.

{bmc LINE.BMP}

# $ K No Ink Cartridge
The ink cartridge is not installed in the printer. 
Complete the installation process for the selected printer.

{bmc LINE.BMP}

# $ K Server Error
A communication problem exists between the HP JetDirect print server and the file server.

{bmc LINE.BMP}

# $ K Resetting Printer
The printer has been reset.
Wait a few minutes for the message to change.

{bmc LINE.BMP}

# $ K Warming Up
The printer is warming up. Wait a few minutes until the message changes.
If the message persists for over 3 minutes, service may be required.

{bmc LINE.BMP}

# $ K + To Change Printer Settings
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the tab for the type of setting you want to change.
3	Select the new settings.
4	Repeat steps 2 and 3 for any other settings.
5	Click OK to activate your selections.

Note
To change printer settings, you must have supervisor rights on one of the file servers that the interface is configured to service.

{bmc LINE.BMP}

# $ K + To View Printer Status
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the Printer tab.
The printer status is shown on the left side of this page.
3	Click OK when you are finished.

See Also
Printer Status

{bmc LINE.BMP}

# $ K Printer Status
Lists the current status of the printer. The status is made up of three items:

{bmc BLTBLK.BMP}	Status Message - Lists the current status of the printer such as online or offline.
{bmc BLTBLK.BMP}	Printer Message - Lists the printer message currently displayed on the printer control panel.
{bmc BLTBLK.BMP}	Traffic Light Icon - Displays 1 of 3 states representing the current state of the printer.

{bmc LINE.BMP}

# $ K Traffic Light Icon
{bmc GO_UP.BMP}  Displays 1 of 3 states representing the current state of the printer:

{bmc BLTBLK.BMP}	Red: A critical error condition exists on the printer which requires user interaction with the printer to continue printing.
{bmc BLTBLK.BMP}	Yellow: A non-critical error condition exists on the printer, but the printer does not require immediate attention.
{bmc BLTBLK.BMP}	Green: The printer is ready to print.

{bmc LINE.BMP}

# $ K + To View Printer Capabilities
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the Printer tab.
Printer capabilities are shown on the lower right side of this page. Capabilities currently installed in the printer may include PCL, PostScript, PowerSave mode, and other capabilities. 
3	Click OK when you are finished.

{bmc LINE.BMP}

# $ K + To Access Property Pages
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the tab for the property page you want displayed.

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Click Help for additional information on the currently displayed property page.

{bmc LINE.BMP}

# $ K To View the Printer Model
1	With the printer highlighted in the list of available printers, click Printer at the top of the main window, then click Properties. 
The available property pages appear.
2	Click the Printer tab.
The currently selected printer model and icon is shown on the upper-right side of this page.
3	Click OK when you are finished.

{bmc LINE.BMP}

# $ K + Printer Property Page

Lists the printer status, model, capabilities, and a brief description of the selected printer. 

See Also
{bmc BUTTON.BMP}	Graphical Printer Status
{bmc BUTTON.BMP}	Printer Status

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K + Page Control Property Page

From this page you can set printer page control selections remotely, including the following items:

{bmc BUTTON.BMP}	Manual Feed
{bmc BUTTON.BMP}	Output Bin
{bmc BUTTON.BMP}	Job Offset

Hints
{bmc BLTBLK.BMP}	These selections change the default settings in the printer, not settings on a per job basis.
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Select Manual Feed
1	With the property pages displayed, click the Page Control tab.
2	Check ON under Manual Feed to enable manual feed or check OFF to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select the Output Bin
1	With the property pages displayed, click the Page Control tab.
2	Check the appropriate output bin.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Job Offset
1	With the property pages displayed, click the Page Control tab.
2	Check On under Job Offset to enable Job Offset or check Off to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Page Setup Property Page

From this page you can remotely configure the printing attributes of the printer including the following selections:

{bmc BUTTON.BMP}	Orientation
{bmc BUTTON.BMP}	Number of Copies
{bmc BUTTON.BMP}	Form Lines
{bmc BUTTON.BMP}	Two-Sided Printing
{bmc BUTTON.BMP}	Paper Size

Hints
{bmc BLTBLK.BMP}	These selections change the default settings in the printer, not settings on a per job basis.
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Select the Page Orientation
1	With the property pages displayed, click the Page Setup tab.
2	To print across the width of your paper, check Portrait under Orientation.
	{bmc port.bmp}
3	To print across the length of your paper, check Landscape under Orientation.
	{bmc land.bmp}
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select the Number of Copies
1	With the property pages displayed, click the Page Setup tab.
2	Use the scroll buttons in the Copies box to select the number of copies desired.
You can also highlight the Copies box and type in the number of copies desired.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select the Number of Form Lines
1	With the property pages displayed, click the Page Setup tab.
2	Use the scroll buttons in the Form Lines box to select the number of lines per page desired.
You can also highlight the Form Lines box and type in the number of lines per page desired.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Two-Sided Printing and Binding Options
1	With the property pages displayed, click the Page Setup tab.
2	To print on both sides of the paper so that pages can be bound along the length of the sheet, check Long Edge Binding under Two-Sided Printing.
	{bmc BINDLONG.BMP}
3	To print on both sides of the paper so that pages can be bound along the width of the sheet, check Short Edge Binding under Two-Sided Printing.
	{bmc BINDSHRT.BMP}
4	To disable two-sided printing, check None.
5	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Your Paper Size
1	With the property pages displayed, click the Page Setup tab.
2	Select the down arrow in the Paper Size box.
3	Select the paper size you want.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Print Quality Property Page

From this page you can remotely configure print quality attributes of the printer including the following selections:

{bmc BUTTON.BMP}	Resolution Enhancement (REt)
{bmc BUTTON.BMP}	Resolution
{bmc BUTTON.BMP}	Economy Mode
{bmc BUTTON.BMP}	Density

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Set Resolution Enhancement (REt)
1	With the property pages displayed, click the Print Quality tab.
2	Select the down arrow in the Resolution Enhancement (REt) box.
3	Select the Resolution Enhancement setting you desire.
4	Click OK to activate your selection.
5	Verify the setting by printing a self-test page and examining the REt pattern on the printout. If required, select a different setting.

Hints
Since the print density and REt setting may affect each other, it is a good practice to adjust both of them at the same time.

{bmc LINE.BMP}

# $ K Resolution Enhancement (REt)
Resolution Enhancement technology (REt) refines the print quality of characters and graphics by smoothing the fine gradations along the angles and curves of the printed image. For optimum print quality, print a self-test page for each available REt setting, then select the setting in which the shading of the REt pattern of the printout is most nearly uniform.
The optimum setting for REt varies over the life of the printer. For optimum print quality, you may occasionally need to change the REt setting.

{bmc LINE.BMP}

# $ K To Set Resolution
1	With the property pages displayed, click the Print Quality tab.
2	Check the Resolution setting (dots per inch) you desire.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Economy Mode
1	With the property pages displayed, click the Print Quality tab.
2	Check On below Economy Mode to enable the mode or OFF to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Errors Property Page

From this page you can select how the printer handles certain error conditions including the following conditions:

{bmc BUTTON.BMP}	PostScript Jam Recovery
{bmc BUTTON.BMP}	Clearable Warnings
{bmc BUTTON.BMP}	Non-Critical Errors (Auto Continue)

This page also displays an error log which lists the last 5 error conditions that occurred in the currently selected printer.

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Set Non-Critical Error Handling
1	With the property pages displayed, click the Errors tab.
2	Check On under Auto Continue to have non-critical error messages appear for 10 seconds before the printer resumes printing.
3	Check Off under Auto Continue to require the user to acknowledge non-critical error messages by pressing Continue on the printer before the printer resumes printing.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Set Clearable Warning Handling
1	With the property pages displayed, click the Errors tab.
2	Check On under Clearable Warnings to have clearable warning messages remain on the printer control panel until they are acknowledged by the user.
3	Check Off under Clearable Warnings to have clearable warning messages remain on the printer control panel until the end of the current print job.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select PostScript Jam Recovery
1	With the property pages displayed, click the Errors tab.
2	Check On under PostScript Jam Recovery to have the printer reprint jammed pages once a paper jam has been cleared.
Setting Jam Recover On impacts printer performance.
3	Check Off under PostScript Jam Recovery to have the printer continue without reprinting jammed pages when a paper jam is cleared.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Advanced Property Page

From this page you can configure the operation of the selected printer including the following items:

{bmc BUTTON.BMP}	Printer Personality
{bmc BUTTON.BMP}	Power Save Mode
{bmc BUTTON.BMP}	Asset Number
{bmc BUTTON.BMP}	Printer Control Panel Language
{bmc BUTTON.BMP}	Timeout

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Select the Printer Personality
1	With the property pages displayed, click the Advanced tab.
2	Select the down arrow in the Personality Control box.
3	Select the appropriate printer personality or click Automatic to enable switching by file type or PJL description.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Power Save Mode
1	With the property pages displayed, click the Advanced tab.
2	Click the down arrow in the Power Save box.
3	Click the amount of time you want the printer to wait since the last print job before going into the reduced power consumption mode or click Off to disable the Power Save mode.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K Power Save Mode
To reduce the amount of power your printer consumes, Power Save shuts down the printer's fuser after the printer has been idle for a specified amount of time (15 minutes to 3 hours). 
When the printer is in Power Save Mode, the printer control panel displays a message indicating it is this mode (such as 00 POWERSAVE).
The printer automatically exits this mode and warms up when you send a print job to the printer, press a control panel key, load or remove paper, or open the top cover.

{bmc LINE.BMP}

# $ K To Set Printer Timeout
1	With the property pages displayed, click the Advanced tab.
2	Place the mouse cursor on the timeout slider, hold down the left mouse button, then move the slider to the right or left to set Timeout between 15 seconds and 5 minutes.
3	Release the mouse button. 
The current setting is displayed at the bottom, center of the box.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Set Print Density
1	With the property pages displayed, click the Print Quality tab.
2	Place the mouse cursor on the density slider, hold down the left mouse button, then move the slider to the right or left to set density between 1 to 5.
3	Release the mouse button.
4	Click OK to activate your selection.

Hints
{bmc BLTBLK.BMP}	You may need to print several pages before the effects of the new setting can be seen. 
{bmc BLTBLK.BMP}	Since the print density and Resolution Enhancement (REt) settings may affect each other, it is a good practice to adjust both of them at the same time.

{bmc LINE.BMP}

# $ K To Select the Printer Display Language
1	With the property pages displayed, click the Advanced tab.
2	Click the down arrow in the Control Panel Language box.
3	Click the language you want the printer to use for control panel messages and text in printer generated pages such as the self-test page.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Assign an Asset Number
1	With the property pages displayed, click the Advanced tab.
2	Click the Asset Number box.
3	Type in an asset number of up to 8 characters for the currently selected printer.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Resources Property Page

From this page you can remotely configure printer selections related to printer memory including the following items:

{bmc BUTTON.BMP}	Image Adapt
{bmc BUTTON.BMP}	Resource Saving
{bmc BUTTON.BMP}	IO Buffering
{bmc BUTTON.BMP}	Page Protection

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Select Image Adapt
1	With the property pages displayed, click the Resources tab.
2	Check Automatic below Image Adapt to enable Image Adapt or check Off to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Resource Saving
1	With the property pages displayed, click the Resources tab.
2	Check Automatic below Resource Saving to enable Resource Saving or check Off to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select I/O Buffering
1	With the property pages displayed, click the Resources tab.
2	Check Automatic below IO Buffering to enable I/O buffering or check Off to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Select Page Protection
1	With the property pages displayed, click the Resources tab.
2	Click the down arrow in the Page Protection box.
3	Select the setting you desire or select Off to disable page protection.
4	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K + Security Property Page

From this page you can control printer security including the following items:

{bmc BUTTON.BMP}	Printer Control Panel Lock
{bmc BUTTON.BMP}	Password

Hints
{bmc BLTBLK.BMP}	To access property pages from the printer list, double-click the printer you want.
{bmc BLTBLK.BMP}	Selections on property pages that are grayed out are not available for the currently selected printer.

{bmc LINE.BMP}

# $ K To Set Printer Control Panel Lock
1	With the property pages displayed, click the Security tab.
2	Check Lock under Control Panel Lock to prevent users from changing settings through the printer control panel or check Unlock to disable the lock function.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K To Enable or Disable the Printer Password
1	With the property pages displayed, click the Security tab.
2	Check Enable to enable password security or check Disable to disable it.
3	Click OK to activate your selection.

{bmc LINE.BMP}

# $ K Manual Feed Needed
The current print job has requested manual feed.
Place a sheet of the appropriate size media (paper) in the manual feed slot of the currently selected printer.

{bmc LINE.BMP}

# $ K Intervention Needed
The printer requires user intervention to correct the current problem. 
This message may indicate the printer is out of paper or offline, or that an I/O error occurred.

{bmc LINE.BMP}

# $ K Status Unknown
No status is currently available for the selected printer.
This is a temporary condition for the printer. It should clear itself soon.
This message may be due to a lack of support in the HP JetDirect print server in the current operating mode.

{bmc LINE.BMP}

# 
Tips gives a brief description of the tasks you can perform on the currently displayed page or window.

# 
Clicking this button closes the currently displayed page or window.

# 
Click Help to access online documentation for tasks and features for the currently displayed page or window.

# 
Click Cancel to cancel all changes made since the last time changes were saved by clicking OK.

# 
Click OK to apply all setting changes made since the last time changes were saved.

# $ K Image Adapt
Image Adapt compresses data to print complete graphics images at 300 dpi using the printer's base memory.
With Image Adapt set to Automatic, the compression routine is applied only to the most complex pages. This may produce a small loss of graphic detail.
With Image Adapt set to Off, the printer prints as much of the image as possible without loosing any detail. Part of the image may be cut off.
Image Adapt is not available on all printers. 

{bmc LINE.BMP}

# $ K Paper Size
Selects the printer's default paper or envelope size. These include the following sizes depending on the printer model you have selected:

Paper Sizes:
11x17 	11 x 17 inches (297 x 432 mm)
A3		297 x 420 mm  (11.7 x 16.5 inches)
A4 		210 x 297 mm  (8.3 x 11.7 inches)
Executive 	7.25 x 10.5 inches  (184 x 267 mm)
JIS B4	250 x 353 mm  (9.8 x 13.9 inches)
JIS B5	176 x 250 mm  (6.9 x 9.8 inches)
Letter 	8.5 x 11 inches (216 x 279 mm)
Legal 	8.5 x 14 inches (216 x 356 mm)

Envelope Sizes:
C5		162 x 229 mm  (6.38 x 9.01 inches)
Com-10	4.12 x 9.5 inches (105 x 241 mm)
DL		110 x 220 mm  (4.33 x 8.66 inches)
Monarch	3.87 x 7.5 inches  (98 x 191 mm)

Your Windows application may override this setting. Before printing, check the paper size selected in your application.

{bmc LINE.BMP}

# 
This graphic enables you to view the current status of the printer at a glance through a graphical representation of the printer's status.

# 
The stoplight displays 1 of 3 states representing the current state of the printer: red indicates a critical error condition, yellow indicates a non-critical error, and green indicates the printer is ready.

# 
Lists the current status of the printer such as online or offline.

# 
Lists the printer message currently displayed on the printer control panel.

# 
Shows the model and icon for the currently selected printer.

# 
Describes the currently selected printer, including its location, installed options, and other information. This information is optional and is input by the network administrator during printer configuration.

# 
Lists the capabilities currently installed in the printer including PCL, PostScript, Power Save mode, and other capabilities.

# 
Click this button to search for a file or directory by browsing a disk and its directory structure.

# 
With manual feed set to On, the printer goes offline when it receives a print job and displays a "manual feed" message. When the user places a sheet of paper in the manual feed input, the printer goes back online and prints.

# 
Use these options to select which bin the printed pages from the printer go to. The available output bins will vary depending on which printer you have selected and which options are available for that printer.

# 
With Job Offset set to On, print jobs are "staggered" as they are placed in the upper output bin to make it easier to locate and separate print jobs.

# 
Select Portrait orientation to print a page that is taller than it is wide. Select Landscape orientation to print a page that is wider than it is tall.

# 
Use these options to select how pages go together when you are printing on both sides of the paper. Long Edge Binding prints the page so it can be bound along the long edge of the paper. Short Edge Binding prints the page so it can be bound across the short edge of the paper.

# 
Lists general printing settings such as the number of copies to print and the number of form lines or lines per page.

# 
Sets the default number of uncollated copies that you want the printer to print. These copies are not sorted. Multiple copies of page 1 are printed, then multiple copies of page 2, and so on.

# 
Form lines sets the vertical spacing (number of lines per page), from 5 to 128, for the default paper size. The factory default is 60 for Letter and 64 for A4-size paper.

# 
Click the down arrow in the Paper Size box, then select the default paper or envelope size you want from the list of available paper sizes (Letter, A4, and so on). The available paper and envelope sizes will vary depending on which printer you have selected.

# 
Lists the available Resolution Enhancement (REt) settings for refining the print quality of characters and graphics for increased print quality.

# 
Lists the resolution options for setting the degree of sharpness for printed characters or images in dots per inch (dpi).

# 
Economy mode lowers printing costs by reducing the amount of toner on the printed page, but also reduces print quality. When set to On, the printed image is lighter with output similar to draft mode found on some dot matrix printers.

# 
With PostScript Jam Recovery set to On, the printer reprints jammed pages once the printer jam is cleared. This results in reduced print speed.

# 
Lists the options for Clearable Warnings. Select On to have the messages remain on the printer control panel until they are acknowledged by the user or Off to have them remain on the printer control panel until the end of the current job.

# 
Lists the options for how the printer reacts to non-critical data and printer errors. Select On to have the printer go offline when an error occurs, then go back online after 10 seconds. Select Off to require the user to acknowledge the error at the printer control panel before the printer returns online.

# 
Lists the last 5 errors that occurred in the currently selected printer, such as offline, paper jam, and so on.

# 
Lists the printer personalities (PCL or PostScript) available for the currently selected printer. Select a default personality or select Automatic for the printer to analyze each job and switch personalities automatically.

# 
This setting enables you to select the amount of time the printer waits since the last print data before ending a print job.

# 
This setting enables you to select the amount of time the printer waits since the last print data before ending a print job.

# 
Density is the measure of the darkness of print on a page, with 1 producing the lightest print and 5 producing the heaviest print.

# 
Click the down arrow to select the amount of time the printer waits since the last print job before entering the reduced power consumption mode (Power Save mode).

# 
Click the down arrow, then select the language (English, French, German) that you want the printer to use for control panel messages and text in printer generated pages such as the self-test page.

# 
This setting enables you to assign a user-defined asset number of up to 8 characters to the printer.

# 
Image Adapt compresses data to print complete graphic images using the printer's base memory. When set to Automatic, complex graphics may be printed with a small loss of graphic detail. When set to Off, no detail is lost, but part of the image may be cut off.

# 
With I/O Buffering set to Automatic, your printer automatically reserves a portion of its memory to hold jobs in progress. Select Off to disable it.

# 
With 2 or more printer personalities installed in the printer and Resource Saving set to Automatic, the printer reserves a portion of its printer memory for each personality's resources. These resources include downloaded fonts, forms, and macros.

# 
For complex pages, Page Protection reserves additional memory for the page image, allowing the printer to create an entire page image in memory before paper starts through the printer. Selecting On or a page size reduces total printer performance, but ensures the entire page is printed.

# 
This setting enables you to lock out certain printer control panel functions to prevent users from making changes to printer settings that may affect other users on the network.

# 
This setting enables you to lock out users from changing printer defaults through their print data. When enabled, the printer rejects all print commands that attempt to change printer defaults, unless the print commands specify the PJL password.

# $ K Clearable Warnings
A clearable warning indicates that a transient condition occurred in the printer. The printer continues online while the message is displayed in place of the "Ready" message. A clearable warning appears each time the printer alters resolution or page protection (which causes a reconfiguration of memory), aborts a print job due to an invalid or uninstalled personality, or encounters a similar temporary condition. A number of clearable warnings can appear during the course of printing a job.
Although most jobs will print, the printer displays a warning to let you know that changes were made to the printer's configuration to accommodate that printing. These changes may result in some changes in the printed output.

{bmc LINE.BMP}

# $ K Power Save On
The printer is currently in the Power Save mode. 
To reduce the amount of power your printer consumes, Power Save mode shuts down the printer's fuser after the printer has been idle for a specified amount of time (15 minutes to 3 hours). 
To exit this mode, send a print job to the printer, press a control panel key, load or remove paper, or open the top cover. After the printer warms up, the printer will return online.

{bmc LINE.BMP}